---
title: Enable NAT for a subnet · Cloudflare Magic WAN docs
description: Enable static NAT for subnets in Magic WAN Connector to  re-use
  address spaces locally.
lastUpdated: 2025-11-04T17:07:51.000Z
chatbotDeprioritize: false
source_url:
  html: https://developers.cloudflare.com/magic-wan/configuration/connector/network-options/nat-subnet/
  md: https://developers.cloudflare.com/magic-wan/configuration/connector/network-options/nat-subnet/index.md
---

## Overview

Each subnet (directly attached or routed) must use a unique address space within the Magic WAN overlay. Many networks already reuse private RFC 1918 space at different sites. To avoid renumbering and still satisfy the Magic WAN uniqueness requirements, you can enable static network address translation (NAT) for a subnet on a Magic WAN Connector.

With subnet NAT, the Connector performs a static, 1:1 translation between:

* The **local prefix** used inside the site.
* A **NAT prefix** that is advertised into the Magic WAN overlay.

Because the mapping is static, the Connector supports both outbound connections from the site and inbound connections from Magic WAN to the site. Connections do not have to be initiated by hosts behind the Magic WAN Connector.

## How subnet NAT works in Magic WAN

NAT is static and 1:1 between equal-sized prefixes. When you enable NAT for a subnet on a Connector:

* The **local prefix** is the subnet on the LAN side of the Connector.

* The **NAT prefix** is a WAN-facing prefix of the same size.

* The Connector translates addresses 1:1 between the two prefixes:

  * For traffic leaving the site towards Magic WAN, it replaces local addresses with the corresponding NAT addresses.
  * For traffic arriving at the site from Magic WAN, it replaces NAT addresses with the corresponding local addresses.

## Addressing rules

To avoid overlapping addresses in the overlay, Magic WAN enforces the following rules:

* **Uniqueness within a LAN**

  * The local prefix for each subnet must be unique within that LAN on the Connector.
  * You can reuse the same local prefix on a different LAN or on a different site.

* **Uniqueness in the Magic WAN overlay**

  * Every **overlay-facing prefix** must be unique across all sites in your Magic WAN deployment.
  * For a subnet **with NAT enabled**, the overlay-facing prefix is the **NAT prefix**.
  * For a subnet **without NAT**, the overlay-facing prefix is the **local prefix**.

These rules allow you to reuse local space at multiple sites, as long as each subnet in the Magic WAN overlay has a unique overlay-facing prefix.

## Example

Consider a subnet that uses the following prefixes:

* **Local prefix**: `192.168.100.0/24`
* **NAT prefix**: `10.10.100.0/24`

In this case:

* When a host inside the site with address `192.168.100.13` sends traffic into the Magic WAN overlay, the Connector translates the address to `10.10.100.13`.
* When traffic from another site, or from the Internet via Magic WAN, targets `10.10.100.13`, the Connector translates the address back to `192.168.100.13`.

## Configure NAT for subnets

You configure subnet NAT when you create or edit a LAN on a Magic WAN Connector. In the Connector configuration:

* You define the **local prefix** for the subnet on the LAN side.
* You optionally define a **static NAT prefix** of the same size. When present, this prefix becomes the overlay-facing prefix for that subnet.

For step-by-step instructions to configure a LAN and supply a static NAT prefix, refer to:

* [Configure hardware Connector](https://developers.cloudflare.com/magic-wan/configuration/connector/configure-hardware-connector/#create-a-lan)
* [Configure Virtual Connector](https://developers.cloudflare.com/magic-wan/configuration/connector/configure-virtual-connector/#create-a-lan)
