---
title: Configure your Magic WAN Connector to connect via static IP assigment ·
  Changelog
description: Local console access for bootstrapping Magic WAN Connector
chatbotDeprioritize: true
source_url:
  html: https://developers.cloudflare.com/changelog/2025-02-14-local-console-access/
  md: https://developers.cloudflare.com/changelog/2025-02-14-local-console-access/index.md
---

# Changelog

New updates and improvements at Cloudflare.

[Subscribe to RSS](https://developers.cloudflare.com/changelog/rss/index.xml)\
[View all RSS feeds](https://developers.cloudflare.com/fundamentals/new-features/available-rss-feeds/)

![hero image](https://developers.cloudflare.com/_astro/hero.CVYJHPAd_ZEA2nF.svg)

[← Back to all posts](https://developers.cloudflare.com/changelog/)

## Configure your Magic WAN Connector to connect via static IP assigment

Feb 14, 2025

[Magic WAN](https://developers.cloudflare.com/magic-wan/)

You can now locally configure your [Magic WAN Connector](https://developers.cloudflare.com/magic-wan/configuration/connector/) to work in a static IP configuration.

This local method does not require having access to a DHCP Internet connection. However, it does require being comfortable with using tools to access the serial port on Magic WAN Connector as well as using a serial terminal client to access the Connector's environment.

For more details, refer to [WAN with a static IP address](https://developers.cloudflare.com/magic-wan/configuration/connector/configure-hardware-connector/#bootstrap-via-serial-console).
