---
title: Egress IPs · Cloudflare Email security (formerly Area 1) docs
description: When you set up Email security (formerly Area 1) using an inline
  deployment, you need to tell your existing email providers to accept messages
  coming from Email security's egress IP addresses.
lastUpdated: 2025-10-27T15:00:52.000Z
chatbotDeprioritize: false
source_url:
  html: https://developers.cloudflare.com/email-security/deployment/inline/reference/egress-ips/
  md: https://developers.cloudflare.com/email-security/deployment/inline/reference/egress-ips/index.md
---

When you set up Email security (formerly Area 1) using an [inline deployment](https://developers.cloudflare.com/email-security/deployment/inline/), you need to tell your existing email providers to accept messages coming from Email security's egress IP addresses.

Refer to this page for reference on what IP subnet mask ranges to use.

Additional information for O365

Office 365 does not support IPv6 addresses nor the following IPv4 subnet mask ranges:

* `104.30.32.0/19`
* `134.195.26.0/23`

If you use Office 365, you will have to use the broken down `/24` subnet mask IP addresses. Refer to [Office 365 `/24` addresses](#office-365-24-addresses) for a list of supported IPv4 addresses.

## United States

For customers in the United States, enter the following IP addresses:

### IPv4

```txt
52.11.209.211
52.89.255.11
52.0.67.109
54.173.50.115
104.30.32.0/19
158.51.64.0/26
158.51.65.0/26
134.195.26.0/23
```

### IPv6

```txt
2405:8100:c400::/38
```

## Europe

For customers in Europe, add all our US IP addresses. Additionally, you need to add the following IP addresses for our European data centers:

```txt
52.58.35.43
35.157.195.63
```

## India

For customers in India, add all our US IP addresses.

## Australia / New Zealand

For customers in Australia and New Zealand, add all our US IP addresses.

## Office 365 `/24` addresses

Use these IPv4 addresses for Office 365, instead of the `/19` and `/23` subnets:

```txt
104.30.32.0/24
104.30.33.0/24
104.30.34.0/24
104.30.35.0/24
104.30.36.0/24
104.30.37.0/24
104.30.38.0/24
104.30.39.0/24
104.30.40.0/24
104.30.41.0/24
104.30.42.0/24
104.30.43.0/24
104.30.44.0/24
104.30.45.0/24
104.30.46.0/24
104.30.47.0/24
104.30.48.0/24
104.30.49.0/24
104.30.50.0/24
104.30.51.0/24
104.30.52.0/24
104.30.53.0/24
104.30.54.0/24
104.30.55.0/24
104.30.56.0/24
104.30.57.0/24
104.30.58.0/24
104.30.59.0/24
104.30.60.0/24
104.30.61.0/24
104.30.62.0/24
104.30.63.0/24
134.195.26.0/24
134.195.27.0/24
```
