---
title: Default password · Cloudflare One docs
description: Learn how to edit Magic WAN Connector's default password.
lastUpdated: 2025-11-04T17:07:51.000Z
chatbotDeprioritize: false
source_url:
  html: https://developers.cloudflare.com/cloudflare-one/networks/connectors/wan-tunnels/configuration/appliances/maintenance/default-password/
  md: https://developers.cloudflare.com/cloudflare-one/networks/connectors/wan-tunnels/configuration/appliances/maintenance/default-password/index.md
---

Magic WAN Connector ships to you with a default password that enables you to access the hardware box or the virtual machine. Cloudflare recommends that you change this password after the first boot.

## Default password to access hardware Magic WAN Connector

The default password for Magic WAN Connector is the serial number (also known as a Service Tag for Dell devices), all uppercase followed by an `!` (exclamation mark). For example, `A1B2C3D!`

## Default password to access Virtual Connector

The default password for Virtual Connector is the last seven characters of your license key, all uppercase, plus an `!` (exclamation mark).

For example, if your license key is `mconn-abcdefghijklmnopqrstuvwxyz`, your default password will be `TUVWXYZ!`.
