---
title: Changelog · Cloudflare Magic Transit docs
description: Review recent changes to Magic Transit.
lastUpdated: 2025-09-25T14:23:12.000Z
chatbotDeprioritize: false
source_url:
  html: https://developers.cloudflare.com/magic-transit/changelog/
  md: https://developers.cloudflare.com/magic-transit/changelog/index.md
---

[Subscribe to RSS](https://developers.cloudflare.com/changelog/rss/magic-transit.xml)

## 2025-07-30

**Magic Transit and Magic WAN health check data is fully compatible with the CMB EU setting.**

Today, we are excited to announce that all Magic Transit and Magic WAN customers with CMB EU ([Customer Metadata Boundary - Europe](https://developers.cloudflare.com/data-localization/metadata-boundary/)) enabled in their account will be able to access GRE, IPsec, and CNI health check and traffic volume data in the Cloudflare dashboard and via API.

This ensures that all Magic Transit and Magic WAN customers with CMB EU enabled will be able to access all Magic Transit and Magic WAN features.

Specifically, these two GraphQL endpoints are now compatible with CMB EU:

* `magicTransitTunnelHealthChecksAdaptiveGroups`
* `magicTransitTunnelTrafficAdaptiveGroups`

## 2024-12-17

**Establish BGP peering over Direct CNI circuits**

Magic WAN and Magic Transit customers can use the Cloudflare dashboard to configure and manage BGP peering between their networks and their Magic routing table when using a Direct CNI on-ramp.

Using BGP peering with a CNI allows customers to:

* Automate the process of adding or removing networks and subnets.
* Take advantage of failure detection and session recovery features.

With this functionality, customers can:

* Establish an eBGP session between their devices and the Magic WAN / Magic Transit service when connected via CNI.
* Secure the session by MD5 authentication to prevent misconfigurations.
* Exchange routes dynamically between their devices and their Magic routing table.

Refer to [Magic WAN BGP peering](https://developers.cloudflare.com/magic-wan/configuration/manually/how-to/configure-routes/#configure-bgp-routes) or [Magic Transit BGP peering](https://developers.cloudflare.com/magic-transit/how-to/configure-routes/#configure-bgp-routes) to learn more about this feature and how to set it up.

## 2024-10-01

**Early access testing for BGP on CNI 2.0 circuits**

Customers can exchange routes dynamically with their Magic virtual network overlay via Direct CNI or Cloud CNI based connectivity.
